### CRV FEB FPGA Register Map (word addresses)

### 

There are four FPGAs on the FEB (part number xc7s50fgga484-2). The address space for each FPGA is offset by 0x400 from its neighbor. The region 0x300 to 0x3FF broadcasts to all FPFAs simultaneously.

0x000..0x2FF – FPGA1. CMB Inputs 1..4 *connected to HDMI inputs* 1..4

0x400..0x6FF – FPGA2. CMB Inputs 1..4 *connected to HDMI inputs* 5..8

0x800..0xAFF – FPGA3. CMB Inputs 1..4 *connected to HDMI inputs* 9..12

0xC00..0xEFF – FPGA4. CMB Inputs 1..4 *connected to HDMI inputs13*..16

**0x020: I/V ADC Input Multiplexer control register**

Selects which of 16 DAC trim resistors is connected to the lower level 16:1multiplexer. Set Mux enable to 0 before taking SiPM pulsed data. The top level 4:1 mux is controlled by the microprocessor. That mux has no disconnect option. The command Mux n where n is 0..3 chooses which lower level mux is connected to the PGA and 24 bit ADC. The microprocessor command A0 n will display n conversions of the 24 bit ADC.

|  |  |  |
| --- | --- | --- |
| 15..5 | 4 | 3..0 |
| Not Used | Mux Enable | Channel Select |

### **0x022: Read/Write test Counter Bits 31...16**

A write to this address defines the upper 16 bits of the 32 bit test counter.   
A read returns the present value of the upper bits.

### **0x023: Read/Write test Counter Bits 15...0**

A write to this address defines the lower 16 bits of the 32 bit test counter.   
A read to this address displays the value of the lower bits and increments all 32 bits of the counter after the read.

### **0x024: One wire command register**

Bits 0..7: If an individual write transaction is requested, the lower eight bits of this register are sent to the one wire interface.

Bit 8: Start the read temperature sequencer. A complete read temperature sequence will execute when this bit is set. The read value of this bit will return a 0 until the sequence is complete.

Bit 9: Start the read ROM sequencer. A complete ROM read sequence will execute when this bit is set. The read value of this bit will return a 0 until the sequence is complete.

|  |  |  |  |
| --- | --- | --- | --- |
| 15..10 | 9 | 8 | 7..0 |
| Not Used | Read ROM | Read Temperature | Command Byte |

### **0x025: One wire control register**

Bit 0..3: Selects which CMB read data is stored in the register file

Bit 4: Request a write transaction

Bit 5: Request a read transaction

Bit 6: Request a reset transaction

Bit 7: Transaction status. Returns a ‘1’ when transaction is in progress

Bit 15..8: Transaction bitcount (N-1). For a write set to seven. For a 72 bit read set to 71.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 15..8 | 7 | 6 | 5 | 4 | 3..0 |
| Transaction bit count | Busy | Rst | Read | Write | CMB Sel |

**0x026..0x2A: One wire returned data register file**

The contents depend on the specifics of the one wire transaction

**0x044..0x45: Bias bus DACs**

Two 12 bits DACs with a possible span of 0..80V. The coding is straight binary, 0x000 is 0V, 0xFFF corresponds to 80V. Address 0x44 applies to CMB1..2, Address 0x45 applies to CMB 3..4. The maximum voltage is in fact set by the bias generator jumper setting on the board. At the highest position the maximum bias voltage is about 76V.